| VELOSTER(FS) >2013 > G 1.6 GDI > Suspension System > General Information>Specifications |

Specifications
Front Suspension
Item | Specification
Suspension type | MacPherson Strut
Shock absorber | Type | GAS
Coil spring | Gamma 1.6 M/T GDI | Free Height [I.D. color] | 290.8mm (11.4488 in.) Green-White
Gamma 1.6 A/T,DCT GDI | 295.0mm (11.6142 in.) Green-Yellow
Gamma 1.6 M/T T-GDI | 306.4mm (12.0630 in.) Orange-White
Gamma 1.6 A/T T-GDI | 314.6mm (12.3858 in.) Orange-Yellow
Rear Suspension
Item | Specification
Suspension type | Torsion Beam Axle
Shock absorber | Type | Monotube
Coil spring | Gamma 1.6 GDI (M/T, A/T, DCT) | Free Height [I.D. color] | 309.9mm (12.2008 in.) Green-Green
Gamma 1.6 T-GDI (M/T, A/T)
Wheel & Tire
Item | Specification
Wheel | Aluminum | 7.0J * 17
7.5J * 18
Tire | 215/45 R17
215/40 R18
Tire pressure | 2.2kg/cm² + 0.07kg/cm² (32psi+1.0psi)
Wheel Alignment
Item | Specification
Front | Toe-in | Total | 0.1° ± 0.2°
Individual | 0.05° ± 0.1°
Camber angle | -0.5° ± 0.5°
Caster angle | 4.22° ± 0.5°
King-pin angle | 13.96° ± 0.5°
Rear | Toe-in | Total | 0.5° (+0.5° / -0.4°)
Individual | 0.25°(+0.25°/ -0.2°)
Camber angle | -1.5° ± 0.5°
Tightening Torques Front Suspension
Item | Tightening torque (kgf.m)
Nm | kgf.m | lb-ft
Wheel Hub nuts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Lower arm to sub frame (Front) | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Lower arm to sub frame (Rear) | 156.9 ~ 176.5 | 16.0 ~ 18.0 | 115.7 ~ 130.2
Lower arm to front axle | 78.5 ~ 88.3 | 8.0 ~ 9.3 | 57.9 ~ 65.1
Tie rod end castle nut | 23.5 ~ 33.3 | 2.4 ~ 3.4 | 19.4 ~ 24.6
Steering gear box to sub frame | 58.8 ~ 78.8 | 6.0 ~ 8.0 | 43.4 ~ 57.9
Stabilizer bar to stabilizer link | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Stabilizer bar to sub frame | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.8
Stabilizer bar to front strut assembly | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Universal joint to pinion | 32.4 ~ 38.3 | 3.3 ~ 3.8 | 23.9 ~ 27.5
Strut assembly to front axle | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Strut assembly upper mounting nut | 44.1 ~ 58.8 | 4.5 ~ 6.0 | 32.5 ~ 43.4
Sub frame mounting bolt & nut | 156.9 ~ 176.5 | 16.0 ~ 18.0 | 115.7 ~ 130.2
Sub frame stay mounting bolt | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.8
Wheel speed sensor & braket | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Shock absorber self-lock nut | 58.8 ~ 68.6 | 6.0 ~ 7.0 | 43.4 ~ 50.6
Rear Suspension
Item | Tightening torque (kgf.m)
Nm | kgf.m | lb-ft
Wheel Hub nuts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Shock absorber upper mounting bolt | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Shock absorber lower mounting bolt & nut | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Torsion beam axle to body | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Torsion beam axle to rear axle | 49.0 ~ 58.8 | 5.0 ~ 6.0 | 36.2 ~ 43.4
Torsion beam axle to caliper | 63.7 ~ 73.5 | 6.5 ~ 7.5 | 47.0 ~ 54.2
Disc fixing screw | 4.9 ~ 5.9 | 0.5 ~ 0.6 | 3.6 ~ 4.3
Wheel speed sensor & bracket | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Parking brake hose bracket | 9.8 ~ 13.7 | 1.0 ~ 1.4 | 7.2 ~ 10.1