| VELOSTER(FS) >2013 > G 1.6 GDI > Restraint (Advanced) > SRSCM>Schematic Diagrams |

Circuit Diagram (1)
Circuit Diagram (2)
Circuit Diagram (3)
SRSCM Connector terminal
Pin | Function (Connector A) | Pin | Function (Connector B)
1 | Ignition | 1 | Seat belt pretensioner [Driver] High
2 | Telltale lamp | 2 | Seat belt pretensioner [Driver] Low
3 | - | 3 | Side airbag [Passenger] Low
4 | (1st stage) Driver airbag Low | 4 | Side airbag [Passenger] High
5 | - | 5 | Curtain airbag [Driver] High
6 | (2nd stage) Passenger airbag High | 6 | Curtain airbag [Driver] Low
7 | Front impact sensor [Driver] High | 7 | Anchor pretensioner [Driver] High
8 | Front impact sensor [Passenger] High | 8 | Anchor pretensioner [Driver] Low
9 | CAN_High | 9 | -
10 | - | 10 | -
11 | - | 11 | Seat belt buckle switch [Passenger] High
12 | Crash Output | 12 | Seat belt buckle switch [Driver] High
13 | (1st stage) Driver airbag High | 13 | Ground
14 | - | 14 | Seat belt pretensioner [Passenger] High
15 | (2nd stage) Passenger airbag Low | 15 | Pressure side impact sensor [Driver] High
16 | Front impact sensor [Driver] Low | 16 | Pressure side impact sensor [Passenger] High
17 | Front impact sensor [Passenger] Low | 17 | Side airbag [Driver] Low
18 | CAN_Low | 18 | Curtain airbag [Passenger] High
19 | - | 19 | Side impact sensor [Passenger] High
20 | - | 20 | Side impact sensor [Driver] High
21 | - | 21 | Anchor pretensioner [Passenger] High
22 | (1st stage) Passenger airbag High | 22 | -
23 | (1st stage) Passenger airbag Low | 23 | -
24 | - | 24 | Seat belt buckle switch [Passenger] Low
25 | - | 25 | Seat belt buckle switch [Driver] Low
26 | - | 26 | -
27 | - | 27 | Seat belt pretensioner [Passenger] Low
|  | 28 | Pressure side impact sensor [Driver] Low
|  | 29 | Pressure side impact sensor [Passenger] Low
|  | 30 | Side airbag [Driver] High
|  | 31 | Curtain airbag [Passenger] Low
|  | 32 | Side impact sensor [Passenger] Low
|  | 33 | Side impact sensor [Driver] Low
|  | 34 | Anchor pretensioner [Passenger] Low
|  | 35 | -
|  | 36 | -
|  | 37 | -
|  | 38 | -
|  | 39 | -