| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Lighting System > Room Lamp>Repair procedures |

Removal
Vanity Lamp
1. | Disconnect the negative (-) battery terminal.
2. | Remove the vanity lamp assembly after disconnecting the connector.
Tailgate Lamp
1. | Disconnect the tailgate lamp connector and remove the tailgate lamp (A).
Installation
Vanity Lamp
1. | Reconnect the vanity lamp connector.
2. | Install the vanity lamp.
Tailgate Lamp
1. | Reconnect the tailgate lamp connector and install the tailgate lamp.