| VELOSTER(FS) >2013 > G 1.6 T-GDI > Suspension System > Front Suspension System > Front Strut Assembly>Components and Components Location |

Components
• | Tighten under unladen condition
• | Fix the strut rod end and tighten the nut
1. Dust cover 2. Upper mounting nuts 3. Self-lock nut 4. Space 5. Insulator 6. Spring upper seat 7. Spring upper pad | 7. Spring upper pad 8. Dust cover & Bumper rubber 9. Coil spring 10. Spring lower pad 11. Piston rod 12. Strut assembly 13. Spring lower seat