| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body (Interior and Exterior) > Body Dimensions > Interior>Body Repair |

Interior A
Front pillar trim mounting hole (Ø8) | Curtain airbag mounting hole (Ø6.6) | Cowl crossbar mounting hole (Ø12)
Front pillar inner panel tooling hole (Ø6.6) | Front door checker mounting hole (Ø13) | Seat belt upper anchor mounting hole (Ø15)
Seat belt upper anchor mounting hole (Ø15) | Center pillar trim mounting hole (Ø10) | Quarter trim mounting hole (Ø8.5)
Seat belt retractor mounting hole (Ø12) | Seat belt retractor mounting hole (Ø12) | Front door striker mounting hole (Ø13)
Front door striker mounting hole (Ø13) |  |
Interior B
Seat belt upper anchor mounting hole (Ø15) | Seat belt upper anchor mounting hole (Ø15) | Center pillar trim mounting hole (Ø10)
Quarter trim mounting hole (Ø8.5) | Seat belt retractor mounting hole (Ø12) | Seat belt retractor mounting hole (Ø12)
Front door striker mounting hole (Ø13) | Front door striker mounting hole (Ø13) | Rear pillar trim mounting hole (Ø8.5)
Quarter inner lower panel tooling hole (Ø14) | Rear pillar trim mounting hole (Ø8.5) | Luggage side trim mounting hole (Ø8.5)
Rear transverse trim mounting hole (Ø8.5) |  |
Interior C
Front pillar trim mounting hole (Ø8) | Curtain airbag mounting hole (Ø6.6) | Cowl crossbar mounting hole (Ø12)
Front pillar inner panel tooling hole (Ø6.6) | Seat belt upper anchor mounting hole (Ø15) | Seat belt upper anchor mounting hole (Ø15)
Center pillar trim mounting hole (Ø10) | Quarter trim mounting hole (Ø8.5) | Seat belt retractor mounting hole (Ø12)
Seat belt retractor mounting hole (Ø12) | Front seat mounting hole (Ø11) |
Interior D
Seat belt upper anchor mounting hole (Ø15) | Seat belt upper anchor mounting hole (Ø15) | Center pillar trim mounting hole (Ø10)
Quarter trim mounting hole (Ø8.5) | Seat belt retractor mounting hole (Ø12) | Seat belt retractor mounting hole (Ø12)
Rear pillar trim mounting hole (Ø8.5) | Quarter inner lower panel tooling hole (Ø18) | Quarter inner lower panel tooling hole (Ø8.5)
Quarter inner lower panel tooling hole (Ø14) | Rear pillar trim mounting hole (Ø8.5) | Luggage side trim mounting hole (Ø8.5)
Rear transverse trim mounting hole (Ø8.5) | Rear floor panel tooling hole (Ø7) |