| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > BCM (Body Control Module) > IPM (Intelligent integrated Platform Module)>Description and Operation |

Description
IPM Overview The Body Control Module (IPM-Intelligent integrated Platform Module) supplies vehicle occupants with visual and audible information and it controls various vehicle functions. To provide and receive information, the module is interfaced to the vehicle's CAN bus communications network. The IPM provides the following features :
- | Wiper & Washer control
- | Lamp control
- | Buzzer control
- | Timer control
- | Door lock/ unlock control
- | Tailgate release control
- | Turn hazard control
- | RKE control
- | Panic alarm flashing control
CAN Communication Netrwork LIN Communication Netrwork
Functions
1. | Wiper control
A. | Front Wiper Mist Control Function
B. | Front Wiper Intermittent Control Function
C. | Front Wiper Washer Control Function
D. | Front Wiper Washer Control Function
E. | Rear Wiper On Switch Control
F. | Rear Washer Wiper Control
G. | Rear Wiper Intermittent Control
2. | Lamp control
A. | Tail Lamp by Switch Control Function
B. | Tail Lamp by Auto Light Control Function
C. | Tail Lamp by Escort Control Function
D. | Tail Lamp by Welcome Control Function
E. | Tail Lamp Autocut Control Function
F. | Output control of Tail Lamp
G. | Head Lamp Low by Switch Control Function
H. | Head Lamp Low by Escort Control Function
I. | Head Lamp Low by Welcome Control Function
J. | Head Lamp Low by Auto Light Control Function
K. | Head Lamp High by Switch Control Function
L. | Head Lamp High and Low by Passing Switch Control Function
M. | Output Control of Head Lamp Low
N. | Output Control of Head Lamp High
O. | Output Control of Head Lamp High Indicator
P. | EC DRL Lamp Function
Q. | Tail Lamp Control by Auto light Mode Control Function
R. | Head Lamp Low Control by Auto light Mode Control Function
S. | AV Tail Control by Auto Light sensor level Control Function
T. | Front Fog Lamp by Switch Control Function
U. | Rear Fog Lamp by Switch Control Function
V. | Room Lamp On / Off / Decaying Control Function
W. | Tail Gate Lamp On / Off Control Function
3. | Buzzer control
A. | Internal Buzzer Control Function
B. | SBW/ SBR Function
C. | Key Reminder warning(Key Operated Warning) Control Function
D. | RKE Teaching Sound Function
E. | SMK System warning Control Function
4. | Timer control
A. | Rear Defogger Control Function
B. | Power Window Main Timer Control Function
5. | Door lock/ unlock control
A. | Central Door Lock/Unlock Switch Control Function
B. | Centrol Door Lock/Unlock Mechanical Key(Door Key) Control Function
C. | Doors Lock/Unlock by RKE
D. | Doors Lock/Unlock by SMK
E. | Doors Relock by ATWS Function
F. | Doors Lock/Unlock by Auto Door
G. | Doors Unlock by Crash
H. | Doors Unlock by Key Reminder
I. | Dead lock/unlock Function
J. | Doors Unlock by MTS
K. | RKE Door Lock/Unlocking Function
L. | Burglar Alarm Relock Door Lock Control Function
M. | SMK Door Lock/Unlocking Function
N. | Central Door Lock/Unlock Button Control Function
O. | Crash Unlock Control Function
P. | Door Lock by Shift-Lever
Q. | Door Lock by Vehicle Speed
R. | Door Unlock by Shift-Lever
S. | Door Unlock by Key Off
T. | Key Reminder Unlock Function
U. | Dead Lock/Unlock Function
V. | Central Unlocking by EC Unlock Control Function
W. | Priority of Door Lock System
X. | Shift Lever MT Option Function
6. | Tailgate release control
7. | Turn hazard control
A. | Hazard Control Function
B. | Turn Signal Control Function
C. | Flasher Failure Control Function
D. | Burglar Alarm Function
E. | Panic Flashing Control Function
F. | Tailgate Flashing Control Function
G. | RKE Two Turn Unlock Set/Reset Flashing Control Function
H. | Emergency Stop Release Flasher Function
I. | Flasher Function Priority Control Function
8. | RKE control
A. | RF Communication Function
B. | RKE (Transmitter) Function
C. | Two Turn Unlock RKE Set/Reset
D. | Receiver & IPM Control Function
E. | IPM RF Control Function
F. | RKE Teaching
G. | RKE Resynchronization
9. | Panic alarm flashing control
10. | Uesr option
A. | Auto Door Lock/Unlock, Two turn unlock, Horn answer back, Head lamp escort, Auto triple turn